Satellite Accumulation Area (SAA)

This Satellite Accumulation Area (SAA) has been approved by EHS for the collection of **HAZARDOUS WASTE** under the following conditions:

1. **Storage limit:**
   * The SAA may accumulate as much as 55 gallons of non-acute hazardous waste, and/or 1 qt. liquid or 1 kg solid acute hazardous waste at any one time.

1. **Containers:**

* Compatible with the hazardous waste being stored
* Incompatible wastes, or incompatible wastes and materials, must not be placed in the same container. TIP: Use secondary containment for liquid

**Closed during storage except when:**

* Adding or removing or consolidating waste
  + - Temporary venting is necessary
    - To prevent build-up of extreme pressure
    - For proper operation of equipment

1. **Label:**
   * All hazardous waste containers must be labeled as **HAZARDOUS WASTE**.
   * Must indicate the primary hazard (corrosive, reactive, etc.)
   * Indicate the approximate percentages of each component totaling 100%
2. **Pick-Up Request:**
   * Submit waste pick up request via the EHS website (ehs.ua.edu)
3. **Emergency Preparedness:** All SAAs must have access to a:
   * + - Emergency management plan
       - Fire alarm & extinguisher
       - Eyewash station & safety shower
       - Spill kit
       - Communication device
       - Maintain appropriate egress
4. **Exclusions:** 
   * **NO BIOHAZARD** or **RADIOACTIVE** waste may be mixed with or stored in the SAA unless otherwise approved by EHS. If you have questions regarding your mixed waste, please contact EHS.

**In the event of an emergency:**

* Alert others in the area and evacuate if necessary
* Phone emergency responders UAPD (205) 348-5454 and EHS (205)348-5905

Lab Hazardous Waste Manager (Please Print): \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Emergency phone number: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_